**Quality Clauses:**

**Q1. Quality Control**

Supplier must ensure that the clauses associated with this purchase order are flowed down to all its sub-tier suppliers. Supplier is required to direct all its external providers to ensure that the requirements of the final product are met.

**Q-2. Quality System**

The Supplier must have a Quality System consistent with industry standards. Axxis reserves the right to review the Supplier’s Quality system.

**Q-3. Review**

During the performance of this Order, Axxis reserves the right to review; verify and/or analyze the Supplier’s Quality and/or Inspection System and Manufacturing processes at the Supplier’s facilities. An Axxis representative must notify the Supplier forty-eight (48) hours in advance of the intended review start date and duration. Buyer’s inspection/acceptance of product prior to shipment is not required unless otherwise specified in this Order.

**Q-4 Notification of Process Changes**

Supplier must notify buyer in writing of changes in product and/or process, changes of its own suppliers, changes of manufacturing facility location and, where required, obtain buyer’s written approval.

**Q-5 Notification of Nonconformities**

Supplier must notify Axxis of any process and/or major nonconforming product or sub-component of the product verbally and in writing as soon as the nonconformance is detected. Major nonconformance means the product or a sub-component of the product will not meet a specification.

**Q-6 Requirements for Sampling**

Where the Supplier utilizes sample inspection plans or other statistical techniques, these must be statistically valid. If the sample contains rejected items, the Supplier must, for the rejected feature or parameter, use a documented method, such as 100% screening to assure Axxis that zero rejects are present.

**Q-7. Product Acceptance**

The Supplier must follow all requirements stated on the purchase order, drawing, data specifications and process instructions to ensure product conformity, documentation and records are obtained.

**Q-8 Qualification and Awareness of Personnel**

The Supplier must employ competent personnel to ensure Buyer’s requirements are met. Suppliers must ensure that their employees are aware of their contribution to product or service conformity, their contribution to product safety, and the importance of ethical behavior.

**Q-9. Record Retention**

The Supplier must maintain records regarding Buyer’s purchase order, specifications, drawings, process requirements, inspection/verification instructions and other relevant technical data. Records must be maintained by the Supplier for a minimum of 10 years or as specified by Axxis after which the Supplier agrees to either return or destroy related records.

**Q-10. Approved Suppliers**

When requested by Buyer or its customers, Supplier agrees to exclusively utilize customer or Buyer approved external providers, including process sources (e.g. special processes).

**Q-11. Access to Facilities**

The Supplier agrees to permit access to the Supplier’s facility for surveying/auditing, if needed. The survey/audits may include personnel from Axxis, Buyer’s customer representative and/or regulatory authorities, and must include access to all records applicable to Buyer’s product or orders.

**Q-12. Counterfeit Parts Detection and Avoidance System Requirements**

Supplier must detect and prevent the use of counterfeit, suspect counterfeit, unapproved, or suspect unapproved parts.

**Q13. Supplier Performance Expectations**

Unless otherwise specified, seller agrees to adhere to meeting or exceeding 90% on-time delivery of product and 90% product quality ratings.

**Q-14. Notification of Nonconformance**

Supplier must notify Axxis of any major nonconforming product or sub-component of the product verbally and in writing as soon as nonconformance is detected. Major nonconformance means the product or a sub-component of the product will not meet a specification.

**Q-15. Requirements for Conformance**

Neither surveillance, inspection and/or tests made by Axxis or Buyer’s representatives at either the Supplier’s or Buyer’s facility, nor the Supplier’s compliance with all applicable product assurance requirements relieve the Supplier of the responsibility to furnish items which conform to the requirements of the purchase order.

**Q-16. Special Processes**

The Supplier and any of its subcontractors performing special processes, that are non-standard according to their approved process flow, must submit a certification listing the specification designation/number and that the special process was performed in accordance with such specification.

**Q-17. Traceability requirements**

The Supplier must provide means of end item traceability. The Supplier may use the original manufacture Lot/Date Code/Serial number or their own method for identifying the end item product as required for proper traceability. Serialized shipments must have the serial numbers listed on the shipper and on the corresponding intermediate packaging.

**Q-18. Identification and Revision Status**

The Supplier must maintain the identification and revision status of all documented information provided by Axxis, including but not limited to specifications, drawings, process requirements, inspection/verification instructions and other relevant product/order related documentation.

**Q-19. Calibration**

The Supplier must maintain the calibration of equipment(s) used to manufacture, test, control, monitor, or measure processes. The calibration standards used must be traceable to international or national measurement standards; when no such standards exist, the basis used for calibration or verification is retained as documented information.

**Q-20. Packaging & Shipping**

The Supplier must use special packaging as required on this order, or when not specified, Supplier may use specially designed shipping containers and/or good commercial practices as deemed necessary to prevent shipping damage. As a minimum, the label must contain the following information: Part number and date of manufacture and Buyer’s Order Number.

**Q-21. Supplier Corrective Action**

In response to Buyer-initiated corrective action requests, Supplier must advise Buyer of root cause determination, corrective action taken to prevent recurrence of reported problems and/or discrepancies, and effectively dates of the planned corrective action(s). Supplier must maintain a corrective action system that determines the effectiveness of such corrective actions, and that prevents shipment of nonconforming articles without prior approval from Buyer.

**Q-22. First Article Inspection**

When requested, the Supplier must perform a First Article Inspection (FAI) of one item from the first production lot, or as required by Axxis. The FAI must consist of recorded actual drawing, specification values, and/or requirements (dimensional, test data, processes, drawing notes, etc.) and may be documented on the drawing or on a separate report form. The first article item must be clearly identified by an external identification marking, and a copy of the FAI must accompany the First Article part. Axxis reserves the right to verify any or all of the characteristics documented on the FAI report at the Supplier’s facility.

**Q-23. Source Inspection**

Source Inspection may be conducted by Axxis at the Supplier’s facilities or where designated in this Order prior to shipment. Inspection/test and/or in-process inspection/test of the articles specified in this Order must be performed by the Supplier and may be witnessed by Axxis’s Quality Representative. Prior to fabrication start, the Supplier and Axxis must determine the process steps at which Source Inspection must be conducted. The Supplier must notify Axxis of the scheduled inspection/test five (5) days in advance. The method of product release must be a stamp or signature by Axxis’s Quality Representative on the Supplier’s shipping or inspection documents.

**Q-24. Certification of Material(s) and Process(es)**

When noted on the Purchase Order, the Supplier must submit certifications for raw material (chemical and physical characteristics) and/or processes (stating specification) used in the manufacturing of the item(s). If outside processing is performed; a certification from subcontractor is to be provided. Note: when specified on the Purchase Order, raw material such as titanium, aluminum, etc. must have the appropriate heat lot identified on each piece for heat lot traceability.

**Q-25. Certificate of Conformance**

The Supplier must furnish a Certificate of Conformance either by email or with each delivery attesting that each item of hardware and/or software conforms to all requirements of Axxis’s specification and purchase order and that all required test and inspections have been performed.

**Q-26 Product Disposition**

Supplier must obtain Buyer’s written approval for nonconforming product disposition.

**Q-27 Disclosure of Non-Authorized Parts, Material, or Assemblies**

Seller agrees to disclose to Buyer if they are not authorized for the parts, material or assemblies they are supplying